Wyoming Department of Health
Healthcare Licensing and Surveys
Hathaway Building, 2300 Capitol Avenue, Suite 510, Cheyenne, WY  82002
Fax: (307) 777-7127    Phone: (307) 777-7123
E-mail: plans-ohls@wyo.gov    Website: https://health.wyo.gov/aging/hls/healthcare-facility-construction/
Checklist for Licensure Construction Survey

	[bookmark: _Hlk231282174]Project Number: 20     

	Facility:      
	Prepared by:      
	Date:      



	

To be submitted in writing to Healthcare Licensing and Surveys
two Weeks Before the Project Survey Date.

	Applicable
To Project
	Not Applicable
 to Project

	Notification that the construction is complete and ready for final inspection.  Healthcare Licensing and Surveys will schedule an inspection for the next available date.
	|_|
	|_|

	Request for license application when the facility is new and/or there is a change of name, location, or number of beds.
	|_|
	|_|

	Written facility fire emergency plans. [2006 NFPA 101:18.7]  - (new facilities only)
	|_|
	|_|

	Written facility smoking regulation. [2006 NFPA 101:18.7] - (new facilities only)
	|_|
	|_|

	Building Systems Certifications and Tests
	
	

	Medical gas. [2005 NFPA 99: Chapter 5]
	|_|
	|_|

	Fire Sprinkler System. [2002 NFPA 13: Chapter 16]
	|_|
	|_|

	Fire alarm system record of completion. [2002 NFPA 72: Section 4.5]
	|_|
	|_|

	Electrical Systems: Grounding system testing. [2005 NFPA 99:4.3.3 and 4.3.4]
	|_|
	|_|

	Electrical Systems: Receptacle testing. [2005 NFPA 99:4.3.3 and 4.3.4]
	|_|
	|_|

	[bookmark: Text18]Electrical Systems: Final electrical approval from the electrical inspector having jurisdiction. [AHJ, NFPA 70]
	|_|
	|_|

	Electrical Systems: Isolated electrical power line isolation monitor tests. [2005 NFPA 99:4.3.3 and 4.3.4]
	|_|
	|_|

	Generator startup: On-site installation tests under the building’s primary power failure. [2005 NFPA 110: 7.13] (New installations only)
	|_|
	|_|

	Generator startup: Full load tests with load equal to 100 percent of nameplate rating. [2005 NFPA 110:7.13] (New installations only)
	|_|
	|_|

	Radiation protection. [Physicist’s report]
	|_|
	|_|

	Fire retardant lumber. [2006 NFPA 101:10.2.6]
	|_|
	|_|

	Drapery flame retardancy. [2006 NFPA 101:18.7.5]
	|_|
	|_|

	Cubicle curtain flame retardancy. [2006 NFPA 101:18.7.5]
	|_|
	|_|

	Vinyl wall covering flame spread rating. [2006 NFPA 101:10.2.3]
	|_|
	|_|

	Paneling flame spread rating. [2006 NFPA 101:10.2.3]
	|_|
	|_|

	Folding door flame spread rating. [2006 NFPA 101:10.2.3]
	|_|
	|_|

	Carpet classification critical radiant flux. [2006 NFPA 101:10.2.7]
	|_|
	|_|

	Sanitization of domestic water piping systems.  [Contractor certification that piping was flushed with sanitizing solution.]
	|_|
	|_|

	Ventilation Balance Report.
	|_|
	|_|

	Final approval from local inspector(s) having jurisdiction.  [AHJ, Insert Codes ]
	|_|
	|_|

	Final approval from Board of Pharmacy inspector(s).
	|_|
	|_|
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